# SoftBank Robotics documentation What's new in NAOqi 2.8?

# Main usages of the Chest button

## When Pepper is off

You may ... | To ... | For further details, see ...
--- | --- | ---
Press once | Turn on | Turning Pepper on
Press and hold for 4 seconds | Update the firmware |

## When Pepper is on

You may ... | To ... | For further details, see ...
--- | --- | ---
Press once | Get IP address, and Read notifications | Requesting technical information
Press again | Skip a message
Press twice | Set the life off and on | Switching Autonomous life on and off
Press and hold for 3 seconds | Shut down | Turning Pepper off
Press and hold for 8 seconds | Request a Forced switch off | Emergency turn off

Glossary Site map Index Support Contact Legal Notices