# SoftBank Robotics documentation What's new in NAOqi 2.8?

# Replacing the battery

See also

Charging the battery

If your battery needs to be replaced:

Step | Action
--- | ---
| Make sure you have a Phillips 0 screwdriver.
| Read the Safety guidelines.
| Disconnect the power cable from the plug located on NAO‘s back.
| Remove the 2 screws of the battery cover with the Phillips 0 screwdriver.
| Remove the used battery and replace it with a new one.
| Once it fits snuggly in its slot, place the cover back into position and tighten all screws.
| Charge your new battery. For further details, see Charging the battery.

Glossary Site map Index Support Contact Legal Notices