# SoftBank Robotics documentation What's new in NAOqi 2.8?

# Loudspeakers

## Specification

Loudspeakers | x2 lateral
Nominal Diameter | 25 mm
Impedance | 8 ohms
Sensitivity | 78dB 1W/1m @ 1 kHz
Input power (nominal) | 5 W
Input power (peak) | 20 W
Frequency Response (-10dB) | 70 Hz - 7.2 kHz

## Location

Part | Name
--- | ---
A | SpeakerLeft
B | SpeakerRight

Glossary Site map Index Support Contact Legal Notices