# SoftBank Robotics documentation What's new in NAOqi 2.8?

# Restore my robot user data

## 1/5 - Making the robot ready for restoration

Step | Action
--- | ---
| Make sure your robot is in version 2.3 or higher. For further details, see: Upgrading my NAO.
| Check the battery level. Important: make sure the robot battery is fully charged: a power shortage during restoring could leave the robot in a fatal state. Tips: if your battery has a limited capacity, you should leave the charger plugged during the upgrade. However it could be wise to order a new battery.
| Make sure you have installed Choregraphe suite. For further details, see: Choregraphe suite - Installation Guide.
| Launch Memory Backup.

## 2/5 - Select the task to perform

Step | Action
--- | ---
| Select Restore .... Warning This action will replace some data on the robot by the ones present in the backup file. It cannot be reverted.
| Click the Next button.

## 3/5 - Connecting to the robot

Step | Action
--- | ---
| Select a robot in the list, or type his IP address. Then click the Next button.
| Enter the password of the robot.
| Click the Connect button.
| Click the Next button.

## 4/5 - Selecting the file to restore

Step | Action
--- | ---
| Use the Browse button to select the backup file to restore on the robot.
| Then click the Next button.

## 5/5 - Finalize the restoration

Step | Action
--- | ---
| Read it carefully and then click the Restore button. Note You will not be able to pursue if the robot is not plugged.
| Once the restoration is done, click the Finish button.

See also Backup/Restore robot data troubleshooting.

Glossary Site map Index Support Contact Legal Notices